<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="69.85" x2="2.54" y2="29.21" width="0" layer="20"/>
<wire x1="2.54" y1="29.21" x2="6.35" y2="25.4" width="0" layer="20" curve="90"/>
<wire x1="6.35" y1="25.4" x2="78.74" y2="25.4" width="0" layer="20"/>
<wire x1="78.74" y1="25.4" x2="82.53" y2="29.19" width="0" layer="20" curve="90"/>
<wire x1="82.53" y1="29.19" x2="82.53" y2="69.87" width="0" layer="20"/>
<wire x1="82.53" y1="69.87" x2="79.07" y2="73.33" width="0" layer="20" curve="90"/>
<wire x1="79.07" y1="73.33" x2="6.02" y2="73.33" width="0" layer="20"/>
<wire x1="6.02" y1="73.33" x2="2.54" y2="69.85" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
<description>SOD-323 (Small Outline Diode)</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
<description>&lt;h3&gt;Plated Through Hole - 2x3 No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-MINIB">
<description>&lt;h3&gt;USB Type Mini-B Surface Mounted&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5 main, 4 shield pins&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/miniUSB-Dimensional.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_Mini-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;h3&gt;HC49/US 11.6x4.6mm PTH Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/Web%20Export/Supplier%20Content/Citizen_300/PDF/Citizen_HC49US.pdf?redirected=1"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MLF44">
<description>&lt;b&gt;44M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
</packages>
</library>
<library name="bt_regulator">
<description>&lt;b&gt;Common Voltage Regulators&lt;/b&gt;
&lt;p&gt;Created by Michael Shimniok &lt;a href="http://www.bot-thoughts.com/"&gt;www.bot-thoughts.com&lt;/a&gt;&lt;/b&gt;</description>
<packages>
<package name="SOT-223-3">
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="QFN-44-NOPAD">
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SKHMPXE010">
<description>&lt;b&gt;6.2 X 6.5mm TACT Switch (SMD)&lt;/b&gt;&lt;p&gt;
Source: http://www3.alps.co.jp/WebObjects/catalog.woa/PDF/E/Switch/Tact/SKHM/SKHM.PDF</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="MINIMELF">
<description>&lt;b&gt;Mini Melf Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-10300"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.3V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-11284"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.3V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-11284"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3-NS" value="SPI_PROG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03" value="self-program">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X03" value="5V/3.3V select">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X03" value="TX-RX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X04_LONGPADS" value="I2C">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X04_LONGPADS" value="I2C">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X06_LONGPADS" value="EXT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X06_LONGPADS" value="EXT2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="USB-MINIB" value="USB_MINI-B_SMT">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08193"/>
<attribute name="SF_ID" value="PRT-00587"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="USB-MINIB" value="USB_MINI-B_SMT">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08193"/>
<attribute name="SF_ID" value="PRT-00587"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_0805" value="green">
<attribute name="LED1" value=""/>
</element>
<element name="LED2" library="led" package="CHIPLED_0805" value="red">
<attribute name="LED2" value=""/>
</element>
<element name="LED3" library="led" package="CHIPLED_0805" value="green">
<attribute name="LED3" value=""/>
</element>
<element name="PWR" library="led" package="CHIPLED_0805" value="PWR">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-Clocks" package="HC49US" value="12Mhz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-Clocks" package="HC49US" value="16Mhz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="68">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603" value="4K7">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603" value="4K7">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603" value="4K7">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="4K7">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603" value="2K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="68">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0603" value="10K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="0603" value="1K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="2.2k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="2K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="2K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="10K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603" value="2K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603" value="68">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603" value="68">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="PD3" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="_PD6" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="atmel" package="MLF44" value="M32L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA32-16MU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1455108"/>
<attribute name="OC_NEWARK" value="58M3733"/>
</element>
<element name="U2" library="bt_regulator" package="SOT-223-3" value="TC1262_VDB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-IC-Microcontroller" package="QFN-44-NOPAD" value="32U4">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-10828"/>
</element>
<element name="LED5" library="led" package="CHIPLED_0805" value="PWR">
<attribute name="VALUE"/>
</element>
<element name="R24" library="SparkFun-Resistors" package="0603" value="2K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="0603" value="2K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="CHIPLED_0805" value="green">
<attribute name="LED4" value=""/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X03" value="L_PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="1X03" value="U_PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch" package="SKHMPXE010" value="SKHMPSE010">
<attribute name="NAME"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="2X3-NS" value="SPI_PROG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="switch" package="SKHMPXE010" value="SKHMPSE010">
<attribute name="NAME"/>
</element>
<element name="PD6" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD5" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD4" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PB4" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PB5" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PB7" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PB6" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ6" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ7" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="MINIMELF" value="CD1206-S01575">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="diode" package="MINIMELF" value="CD1206-S01575">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="39"/>
<contactref element="JP1" pad="GND"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="PWR" pad="C"/>
<contactref element="C8" pad="2"/>
<contactref element="JP2" pad="GND"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U3" pad="33"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="15"/>
<contactref element="U3" pad="23"/>
<contactref element="U3" pad="35"/>
<contactref element="U3" pad="43"/>
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="J5" pad="4"/>
<contactref element="J6" pad="4"/>
<contactref element="R23" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="LED5" pad="C"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="5"/>
<contactref element="S1" pad="2"/>
<contactref element="J7" pad="6"/>
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="5"/>
<contactref element="JP2" pad="S2"/>
<contactref element="JP2" pad="S4"/>
<contactref element="JP2" pad="S1"/>
<contactref element="JP2" pad="S3"/>
<contactref element="JP1" pad="S2"/>
<contactref element="JP1" pad="S4"/>
<contactref element="JP1" pad="S1"/>
<contactref element="JP1" pad="S3"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="D-"/>
<contactref element="D2" pad="C"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="D+"/>
<contactref element="D1" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="7"/>
<contactref element="Q1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="8"/>
<contactref element="Q1" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="R5" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R4" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="24"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="40"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="4"/>
<contactref element="R6" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="S2" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="SJ7" pad="1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="23"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$11">
<contactref element="PWR" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="VBUS"/>
<contactref element="J3" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="JP2" pad="VBUS"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="7"/>
<contactref element="SJ1" pad="2"/>
<contactref element="SJ2" pad="1"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="J3" pad="3"/>
<contactref element="U2" pad="3"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="JP2" pad="D+"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R8" pad="2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="U3" pad="3"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="R9" pad="1"/>
<contactref element="JP2" pad="D-"/>
</signal>
<signal name="N$18">
<contactref element="Q2" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U3" pad="17"/>
</signal>
<signal name="N$19">
<contactref element="Q2" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="N$21">
<contactref element="U3" pad="6"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U3" pad="42"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="J5" pad="3"/>
<contactref element="R11" pad="1"/>
<contactref element="U3" pad="18"/>
</signal>
<signal name="N$27">
<contactref element="R10" pad="1"/>
<contactref element="J5" pad="2"/>
<contactref element="U3" pad="19"/>
</signal>
<signal name="N$26">
<contactref element="J6" pad="3"/>
<contactref element="R13" pad="1"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="N$31">
<contactref element="R14" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$32">
<contactref element="LED3" pad="C"/>
<contactref element="U3" pad="32"/>
</signal>
<signal name="RT1">
<contactref element="J4" pad="3"/>
<contactref element="SJ4" pad="2"/>
<contactref element="SJ6" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="U3" pad="10"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="N$33">
<contactref element="U3" pad="9"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="44"/>
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="U3" pad="27"/>
<contactref element="C14" pad="2"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C14" pad="1"/>
<contactref element="SJ7" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="30"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="31"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="32"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="N$41">
<contactref element="U1" pad="33"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="N$42">
<contactref element="U1" pad="34"/>
<contactref element="J8" pad="5"/>
</signal>
<signal name="N$43">
<contactref element="U1" pad="35"/>
<contactref element="J8" pad="6"/>
</signal>
<signal name="N$46">
<contactref element="U3" pad="36"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="U3" pad="37"/>
<contactref element="J9" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="U3" pad="38"/>
<contactref element="J9" pad="3"/>
</signal>
<signal name="N$49">
<contactref element="U3" pad="39"/>
<contactref element="J9" pad="4"/>
</signal>
<signal name="N$50">
<contactref element="U3" pad="40"/>
<contactref element="J9" pad="5"/>
</signal>
<signal name="N$51">
<contactref element="U3" pad="41"/>
<contactref element="J9" pad="6"/>
</signal>
<signal name="N$61">
<contactref element="U1" pad="15"/>
<contactref element="PD6" pad="1"/>
</signal>
<signal name="N$62">
<contactref element="U1" pad="14"/>
<contactref element="PD5" pad="1"/>
</signal>
<signal name="N$64">
<contactref element="U1" pad="12"/>
<contactref element="PD3" pad="TP"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="41"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$68">
<contactref element="_PD6" pad="TP"/>
<contactref element="U3" pad="26"/>
</signal>
<signal name="N$71">
<contactref element="U3" pad="28"/>
<contactref element="PB4" pad="1"/>
</signal>
<signal name="N$72">
<contactref element="U3" pad="29"/>
<contactref element="PB5" pad="1"/>
</signal>
<signal name="N$73">
<contactref element="LED5" pad="A"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$74">
<contactref element="R25" pad="1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$69">
<contactref element="LED4" pad="C"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="U3" pad="13"/>
<contactref element="R21" pad="1"/>
<contactref element="J7" pad="5"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$29">
<contactref element="U3" pad="11"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="R7" pad="2"/>
<contactref element="J10" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="38"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="17"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="VEE">
<contactref element="R24" pad="2"/>
<contactref element="J11" pad="3"/>
<contactref element="R25" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="J7" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="U3" pad="44"/>
<contactref element="U3" pad="24"/>
<contactref element="U3" pad="34"/>
<contactref element="U3" pad="14"/>
<contactref element="J5" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="VCC">
<contactref element="J3" pad="2"/>
<contactref element="J10" pad="2"/>
<contactref element="J11" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="U3" pad="12"/>
<contactref element="PB7" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="U1" pad="13"/>
<contactref element="PD4" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="U3" pad="30"/>
<contactref element="PB6" pad="TP"/>
</signal>
<signal name="N$38">
<contactref element="U1" pad="9"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="U3" pad="21"/>
<contactref element="SJ6" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="U3" pad="20"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="U1" pad="20"/>
<contactref element="R12" pad="1"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="U1" pad="10"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="RT0">
<contactref element="SJ5" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="SJ3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
