<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="116.916" y1="68.504" x2="69.774" y2="68.504" width="0" layer="20"/>
<wire x1="69.774" y1="68.504" x2="64.77" y2="63.5" width="0" layer="20" curve="90"/>
<wire x1="64.77" y1="63.5" x2="64.77" y2="43.178665625" width="0" layer="20"/>
<wire x1="64.77" y1="43.178665625" x2="69.848665625" y2="38.102221875" width="0" layer="20" curve="90"/>
<wire x1="69.848665625" y1="38.102221875" x2="116.8611" y2="38.118228125" width="0" layer="20"/>
<wire x1="116.8611" y1="38.118228125" x2="121.916015625" y2="43.18015625" width="0" layer="20" curve="90"/>
<wire x1="121.916015625" y1="43.18015625" x2="121.9" y2="63.52" width="0" layer="20"/>
<wire x1="121.9" y1="63.52" x2="116.916" y2="68.504" width="0" layer="20" curve="90"/>
<text>USBtin</text>
<text>PCB by CoSailer</text>
<text>by Thomas Fischl</text>
<text>G    H    L</text>
<text>Bootloader</text>
<text>PWR</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;h3&gt;USB Type Mini-B Surface Mounted&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5 main, 4 shield pins&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/miniUSB-Dimensional.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_Mini-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="DIP254P762X432-18">
</package>
<package name="DIP254P762X533-20">
</package>
<package name="DIP254P762X432-8">
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;h3&gt;HC49/US 11.6x4.6mm PTH Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/Web%20Export/Supplier%20Content/Citizen_300/PDF/Citizen_HC49US.pdf?redirected=1"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-10300"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="22pF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="22puF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="USB-MINIB" value="USB_MINI-B_SMT">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08193"/>
<attribute name="SF_ID" value="PRT-00587"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="120">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Microchip_By_element14_Batch_1" package="DIP254P762X432-18" value="MCP2515-I/P-2">
<attribute name="DESCRIPTION" value="CAN CONTRL"/>
<attribute name="MPN" value="MCP2515-I/P"/>
<attribute name="OC_FARNELL" value="1439391"/>
<attribute name="OC_NEWARK" value="61K2945"/>
<attribute name="PACKAGE" value="PDIP-18"/>
<attribute name="SUPPLIER" value="MICROCHIP"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Microchip_By_element14_Batch_1" package="DIP254P762X533-20" value="PIC18F14K50-I/P-2">
<attribute name="MPN" value="PIC18F14K50-I/P"/>
<attribute name="OC_FARNELL" value="1648501"/>
<attribute name="OC_NEWARK" value="77M3103"/>
<attribute name="PACKAGE" value="DIP-20"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="Microchip_By_element14_Batch_1" package="DIP254P762X432-8" value="MCP2551-I/P-2">
<attribute name="DESCRIPTION" value="CAN CTRL"/>
<attribute name="MPN" value="MCP2551-I/P"/>
<attribute name="OC_FARNELL" value="1292240"/>
<attribute name="OC_NEWARK" value="61K2947"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="HC49US" value="24MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$2" pad="19"/>
<contactref element="J1" pad="D+"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="18"/>
<contactref element="J1" pad="D-"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="VBUS"/>
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U$1" pad="18"/>
<contactref element="R3" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="S1"/>
<contactref element="J1" pad="S2"/>
<contactref element="J1" pad="S3"/>
<contactref element="J1" pad="S4"/>
<contactref element="U$2" pad="20"/>
<contactref element="J2" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U$1" pad="9"/>
<contactref element="J4" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C3" pad="1"/>
<contactref element="U$2" pad="17"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="4"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="12"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="6"/>
<contactref element="U$1" pad="17"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="12"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="16"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="D1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$2" pad="13"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="N$12">
<contactref element="U$2" pad="11"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="N$13">
<contactref element="U$3" pad="4"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$3" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U$3" pad="8"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="8"/>
<contactref element="C7" pad="1"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="7"/>
<contactref element="C6" pad="1"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="11"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="10"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="N$21">
<contactref element="U$3" pad="7"/>
<contactref element="J4" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R4" pad="1"/>
<contactref element="J4" pad="3"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="J3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="14"/>
<contactref element="U$2" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
